**Experiment / Assignment / Tutorial No. 1**

**Grade: AA / AB / BB / BC / CC / CD /DD**

**Signature of the Staff In-charge with date**

|  |
| --- |
| **Batch: B-1 Roll No.: 16010122104 Experiment / assignment / tutorial No.: 1** |

|  |
| --- |
| **Title:** Basic Gates & Universal Gates |

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Objective:** To study the basic gates: AND, OR, NOT and universal gates: NAND, NOR, XOR, XNOR

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Expected Outcome of Experiment:**

**CO1:** Recall basic gates and binary, octal & hexadecimal calculations and conversions.

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Books/ Journals/ Websites referred:**

* Vlab Link: [http://vlabs.iitkgp.ernet.in/dec/#](http://vlabs.iitkgp.ernet.in/dec/)
* R. P. Jain, “Modern Digital Electronics”, Tata McGraw Hill
* http://www.ee.surrey.ac.uk/Projects/Labview/gatesfunc/
* http://www.electronics-tutorials.ws/boolean/bool\_6.html

**Pre Lab/ Prior Concepts:**

Gate is a logic circuit with one or more inputs but only one output. Gates are digital (two state) circuit because the input & output are either low or high. Gates provide high output for certain combinations of input & for other combinations the output is low. Total number of combinations for a gate is 2^n; where n is number of input.

**Classification:** The two types of gate are:

1. **Basic or Fundamental Gates:**
2. **Derived Gates:**

**Symbols of gates**

A diagram of different types of electrical components

Description automatically generated


|  |  |
| --- | --- |
| **Type of IC** | **Specification** |

**Implementation Details:**

**Basic Gates**

1. **OR gate:** The OR gate has two or more inputs but only 1 output. If any or all the inputs are high, the output is high. If all the inputs are low, the output is low.

**Y= A + B**

**Symbol for OR gate** **Pin Diagram For IC 7432**

The truth table for OR operations are:

A table with numbers and symbols

Description automatically generated

1. **AND gate:** The AND gate has two or more inputs but only one output. If any or all inputs are high then output is also high

**Y = A.B**

**Symbol for AND gate** **Pin Diagram For IC 7408**

A diagram of a circuit board

Description automatically generated

The truth table for AND operations are:

A table with numbers and symbols

Description automatically generated

1. **NOT gate:** The Not gate is a gate with only one input and one output. The output is always in opposite state of an input. A NOT gate is also called as Inverter because it performs inversion.

**Y= A’**

A white background with black dots

Description automatically generated

**Symbol for NOT gate** **Pin Diagram For IC 7404**

A diagram of a circuit

Description automatically generated

The truth table for NOT operations is:

A table with numbers and symbols

Description automatically generated

**Derived Gates/Universal Gates**

* + NAND gate
  + NOR gate
  + EX-OR gate
  + EX-NOR gate

1. **NAND gate:** This is a NOT-AND gate which is equal to an AND gate followed by a NOT gate. The outputs of all NAND gates are high if any of the inputs are low. The symbol is an AND gate with a small circle on the output. The small circle represents inversion.

**Y= (A.B)’**

A diagram of a circuit board

Description automatically generated

The truth table for NAND operations is:

A table with numbers and letters

Description automatically generated

1. **NOR gate:** This is a NOT-OR gate which is equal to an OR gate followed by a NOT gate. The outputs of all NOR gates are low if any of the inputs are high. The symbol is an OR gate with a small circle on the output. The small circle represents inversion.

**Y= (A+B)’**

A diagram of a circuit

Description automatically generated

The truth table for NOR operations are:


A table with numbers and symbols

Description automatically generated

1. **EX-OR gate**: The 'Exclusive-OR' gate is a circuit which will give a high output if either, but not both, of its two inputs are high. An encircled plus sign ( ) is used to show the EX-OR operation

Y=A⨁B

**Symbol for Ex-OR gate** **Pin Diagram For IC 7486**



The truth table for XOR operations is:

A table with numbers and symbols

Description automatically generated

1. **EX-NOR gate**: The 'Exclusive-NOR' gate circuit does the opposite to the EOR gate. It will give a low output if either, but not both, of its two inputs are high. The symbol is an EXOR gate with a small circle on the output. The small circle represents inversion

Y=(A⨁B)’

A diagram of an electrical component

Description automatically generated

The truth table for XNOR operations is:

A table with numbers and symbols

Description automatically generated

**Implementation Using NAND Gate**

**NOT GATE STEPS**

A NOT gate is made by joining the inputs of a NAND gate together. Since a NAND gate is equivalent to an AND gate followed by a NOT gate, joining the inputs of a NAND gate leaves only the NOT gate.

A white rectangular object with black lines

Description automatically generated

**AND GATE**

An AND gate is made by inverting the output of a NAND gate as shown below.

A white rectangular object with black text

Description automatically generated

**OR GATE**

If the truth table for a NAND gate is examined or by applying De Morgan's Laws, it can be seen that if any of the inputs are 0, then the output will be 1. To be an OR gate, however, the output must be 1 if any input is 1. Therefore, if the inputs are inverted, any high input will trigger a high output.

A black and white diagram

Description automatically generated with medium confidence


**IMPLEMENTATION USING NOR GATE**

**NOT GATE STEPS**

This is made by joining the inputs of a NOR gate. As a NOR gate is equivalent to an OR gate leading to NOT gate, this automatically sees to the "OR" part of the NOR gate, eliminating it from consideration and leaving only the NOT part.

![A white background with black dots

Description automatically generated](data:image/png;base64,iVBORw0KGgoAAAANSUhEUgAAALoAAAA6CAYAAAAHvkMpAAAAsklEQVR4Xu3SoQEAMAjAMP5/GvxOWBNZ3VkImDfAj4xOgtFJMDoJRifB6CQYnQSjk2B0EoxOgtFJMDoJRifB6CQYnQSjk2B0EoxOgtFJMDoJRifB6CQYnQSjk2B0EoxOgtFJMDoJRifB6CQYnQSjk2B0EoxOgtFJMDoJRifB6CQYnQSjk2B0EoxOgtFJMDoJRifB6CQYnQSjk2B0EoxOgtFJMDoJRifB6CQYnQSjk2B0Eg4xbPE6rAVo5gAAAABJRU5ErkJggg==)



**AND GATE**

An AND gate is made by inverting the output of a NAND gate as shown below.

A table with numbers and letters

Description automatically generated

**OR GATE**

If the truth table for a NAND gate is examined or by applying De Morgan's Laws, it can be seen that if any of the inputs are 0, then the output will be 1. To be an OR gate, however, the output must be 1 if any input is 1. Therefore, if the inputs are inverted, any high input will trigger a high output.

A diagram of a graph

Description automatically generated with medium confidence

**Conclusion:**

**Post Lab Descriptive Questions**

1. Verify the expression (A∙B)' + C by:
2. Using NAND Gate directly.
3. Using AND & NOT gate consecutively.
4. Implement the following expressions using a combination of gates:
5. (A'+B)∙B
6. (A∙B)+A'
7. A∙ (B∙B')
8. (A'⊕B)∙A